% legacy style for circuits --- useful as a base for designing your style
% Do not use LaTeX commands if you want it to be compatible with ConTeXt
% Do not add spurious spaces
%
\tikzset{legacy circuit style/.style={\circuitikzbasekey/.cd,%
% Resistors
resistors/scale=1.0,
resistors/width=0.8,
resistors/zigs=3,
resistors/fill=none,
resistors/thickness=none,
%
% Capacitors
capacitors/scale=1.0,
capacitors/fill=none,
capacitors/thickness=none,
%
% Inductors (and transformers)
inductors/scale=1.0,
inductors/fill=none,
inductors/thickness=none,
% these two are not set because the default is different in american and cute coils
% inductors/width=0.6, % it's 0.8 for american coils
% inductors/coils=5, % it's 4 for american coils
%
% Diodes
diodes/scale=1.0,
diodes/fill=none,
diodes/thickness=none,
%
% Batteries
batteries/scale=1.0,
batteries/fill=none,
batteries/thickness=none,
%
% Independent sources (the round ones)
sources/scale=1.0,
sources/fill=none,
sources/thickness=none,
% Dependent sources (the diamond-shaped ones)
csources/scale=1.0,
csources/fill=none,
csources/thickness=none,
%
% Instruments
instruments/scale=1.0,
instruments/fill=none,
instruments/thickness=none,
%
% Mechanical analogy
mechanicals/scale=1.0,
mechanicals/fill=none,
mechanicals/thickness=none,
%
% Misc component (look at the manual)
misc/scale=1.0,
misc/fill=none,
misc/thickness=none,
%
% Block diagrams
blocks/scale=1.0,
blocks/fill=none,
blocks/thickness=none,
%
% Ground symbols
grounds/scale=1.0,
grounds/fill=none,
grounds/thickness=none,
%
% Power supplies (but look at the manual, you can do more)
power supplies/scale=1.0,
power supplies/fill=none,
power supplies/thickness=none,
%
% Transistors
transistors/scale=1.0,
transistors/fill=none,
transistors/thickness=none,
tripoles/mos style=no arrows,  % it can be "arrows"
tripoles/pmos style=fullcircle, % it can be "fullcircle", "nocircle"
transistors/arrow pos=legacy, % it can be "end"
%
% Vacuum tubes
tubes/scale=1.0,
tubes/fill=none,
tubes/thickness=none,
%
% RF components
RF/scale=1.0,
RF/fill=none,
RF/thickness=none,
%
% Electromechanical
electromechanicals/scale=1.0,
electromechanicals/fill=none,
electromechanicals/thickness=none,
%
% Amplifiers
amplifiers/scale=1.0,
amplifiers/fill=none,
amplifiers/thickness=none,
%
% Switches (they're a bit special, look the manual)
switches/scale=1.0,
switches/fill=none,
switches/thickness=none,
%
% Logic ports
logic ports/scale=1.0,
logic ports/fill=none,
logic ports/thickness=none,
logic ports origin=legacy, % it can be "center" (better)
american or shape=roundy,% could be pointy
%
% flip-flops
flipflops/scale=1.0,
flipflops/fill=none,
flipflops/thickness=none,
%
% Integrated circuits
chips/scale=1.0,
chips/fill=none,
chips/thickness=none,
%
% Displays
displays/scale=1.0,
displays/fill=none,
displays/thickness=none,
%
% Nodes width (connectors, etc
nodes width=.04,
%
% Arrows size
current arrow scale=16,
},% end .style
}% end \tikzset
% You can add more commands here
% Do not use LaTeX commands if you want it to be compatible with ConTeXt
% Do not add spurious spaces
%
\endinput

