
%% Options




%% Keys

\long\def\pgf@circ@comment#1{}

\def\circuitikzbasekey{/tikz/circuitikz}

\pgfkeys{\circuitikzbasekey/.is family}

\def\circuitikzset#1{\pgfkeys{\circuitikzbasekey,#1}}
\let\ctikzset\circuitikzset
\def\ctikzvalof#1{\pgfkeysvalueof{\circuitikzbasekey/#1}}
\def\ctikzsetvalof#1#2{\pgfkeyssetvalue{\circuitikzbasekey/#1}{#2}}

\ctikzset{bipoles/.is family}
\ctikzset{bipoles/border margin/.initial=1.1}
\ctikzset{bipoles/thickness/.initial=2} 
\ctikzset{bipoles/length/.initial=1.4cm} 
\ctikzset{nodes width/.initial=.04}
\newdimen\pgf@circ@Rlen 
\ctikzset{bipoles/length/.code={\pgf@circ@Rlen = #1}} 

\ctikzset{monopoles/.is family}
\ctikzset{monopoles/ground/width/.initial=.25}
\ctikzset{monopoles/chassis/width/.initial=.25}
\ctikzset{monopoles/alternative chassis/width/.initial=.25}
\ctikzset{monopoles/equipotentiality/width/.initial=.25}
\ctikzset{monopoles/tlinestub/width/.initial=.25}          
\ctikzset{monopoles/antenna/width/.initial=.25}            
\ctikzset{monopoles/antenna/label/xanchor/.initial=.4}            
\ctikzset{monopoles/antenna/label/yanchor/.initial=.75}            
\ctikzset{monopoles/txantenna/label/xanchor/.initial=.4}            
\ctikzset{monopoles/txantenna/label/yanchor/.initial=.75}            
\ctikzset{monopoles/txantenna/width/.initial=.25}
\ctikzset{monopoles/rxantenna/label/xanchor/.initial=.4}            
\ctikzset{monopoles/rxantenna/label/yanchor/.initial=.75}            
\ctikzset{monopoles/rxantenna/width/.initial=.25}

\ctikzset{bipoles/resistor/height/.initial=.3}
\ctikzset{bipoles/resistor/width/.initial=.8}
\ctikzset{bipoles/potentiometer/height/.initial=.8}
\ctikzset{bipoles/potentiometer/height 2/.initial=.3}
\ctikzset{bipoles/potentiometer/width/.initial=.8}
\ctikzset{bipoles/photoresistor/height/.initial=.6}
\ctikzset{bipoles/photoresistor/height 2/.initial=.3}
\ctikzset{bipoles/photoresistor/width/.initial=.8}
\ctikzset{bipoles/thermistor/main/.initial=.7}
\ctikzset{bipoles/thermistor/height/.initial=.428}%.3/.7
\ctikzset{bipoles/thermistorntc/width/.initial=.8}
\ctikzset{bipoles/thermistorntc/main/.initial=.7}
\ctikzset{bipoles/thermistorntc/height/.initial=.428}%.3/.7
\ctikzset{bipoles/thermistorntc/height 2/.initial=.75}%.3/.7
\ctikzset{bipoles/thermistorptc/width/.initial=.8}
\ctikzset{bipoles/thermistorptc/main/.initial=.7}
\ctikzset{bipoles/thermistorptc/height/.initial=.428}%.3/.7
\ctikzset{bipoles/thermistorptc/height 2/.initial=.75}%.3/.7
\ctikzset{bipoles/thermistor/width/.initial=.8}
\ctikzset{bipoles/varistor/main/.initial=.7}
\ctikzset{bipoles/varistor/height/.initial=.428}%.3/.7
\ctikzset{bipoles/varistor/width/.initial=.8}
\ctikzset{bipoles/vresistor/height/.initial=.6}
\ctikzset{bipoles/vresistor/width/.initial=.8}
\ctikzset{bipoles/cuteinductor/height/.initial=.3}
\ctikzset{bipoles/cuteinductor/width/.initial=.8}
\ctikzset{bipoles/cuteinductor/coils/.initial=6}
\ctikzset{bipoles/americaninductor/height/.initial=.3}
\ctikzset{bipoles/americaninductor/height 2/.initial=.1}
\ctikzset{bipoles/americaninductor/width/.initial=.8}
\ctikzset{bipoles/americaninductor/coils/.initial=4}
\ctikzset{bipoles/vcuteinductor/height/.initial=.6}
\ctikzset{bipoles/vcuteinductor/coil height/.initial=.3}
\ctikzset{bipoles/vcuteinductor/width/.initial=.8}
\ctikzset{bipoles/vcuteinductor/coils/.initial=6}
\ctikzset{bipoles/vamericaninductor/height/.initial=.6}
\ctikzset{bipoles/vamericaninductor/height 2/.initial=.2}
\ctikzset{bipoles/vamericaninductor/width/.initial=.8}
\ctikzset{bipoles/vamericaninductor/coils/.initial=4}
\ctikzset{bipoles/isource/height/.initial=.60}
\ctikzset{bipoles/isource/width/.initial=.60}
\ctikzset{bipoles/isourceam/height/.initial=.60}
\ctikzset{bipoles/isourceam/width/.initial=.60}
\ctikzset{bipoles/vsource/height/.initial=.60}
\ctikzset{bipoles/vsource/width/.initial=.60}
\ctikzset{bipoles/vsourceam/height/.initial=.60}
\ctikzset{bipoles/vsourceam/width/.initial=.60}
\ctikzset{bipoles/vsourceam/margin/.initial=.7}
\ctikzset{bipoles/isourcesin/height/.initial=.60}
\ctikzset{bipoles/isourcesin/width/.initial=.60}
\ctikzset{bipoles/vsourcesin/height/.initial=.60}
\ctikzset{bipoles/vsourcesin/width/.initial=.60}
\ctikzset{bipoles/vsourcesquare/height/.initial=.60}
\ctikzset{bipoles/vsourcesquare/width/.initial=.60}
\ctikzset{bipoles/cisource/height/.initial=.7}
\ctikzset{bipoles/cisource/width/.initial=.7}
\ctikzset{bipoles/cisourceam/height/.initial=.7}
\ctikzset{bipoles/cisourceam/width/.initial=.7}
\ctikzset{bipoles/cvsource/height/.initial=.7}
\ctikzset{bipoles/cvsource/width/.initial=.7}
\ctikzset{bipoles/cvsourceam/height/.initial=.7}
\ctikzset{bipoles/cvsourceam/width/.initial=.7}
\ctikzset{bipoles/cvsourceam/margin/.initial=.7}
\ctikzset{bipoles/cvsourceam/text scale/.initial=1}
\ctikzset{bipoles/cisourcesin/width/.initial=.7}
\ctikzset{bipoles/cvsourcesin/height/.initial=.7}
\ctikzset{bipoles/cvsourcesin/width/.initial=.7}
\ctikzset{bipoles/capacitor/height/.initial=.6}
\ctikzset{bipoles/capacitor/width/.initial=.2}
\ctikzset{bipoles/pcapacitor/height/.initial=.6}
\ctikzset{bipoles/pcapacitor/width/.initial=.2}
\ctikzset{bipoles/pcapacitor/bend width/.initial=1.1}
\ctikzset{bipoles/vcapacitor/height/.initial=.6}
\ctikzset{bipoles/vcapacitor/width/.initial=.5}
\ctikzset{bipoles/vcapacitor/capacitor width/.initial=.4}
\ctikzset{bipoles/battery/height/.initial=.6}
\ctikzset{bipoles/battery/width/.initial=.3}
\ctikzset{bipoles/battery1/height/.initial=.6}
\ctikzset{bipoles/battery1/width/.initial=.3}
\ctikzset{bipoles/diode/height/.initial=.50}
\ctikzset{bipoles/diode/width/.initial=.40}
\ctikzset{bipoles/varcap/height/.initial=.50}
\ctikzset{bipoles/varcap/width/.initial=.45}
\ctikzset{bipoles/interr/height/.initial=.35}
\ctikzset{bipoles/interr/width/.initial=.35}
\ctikzset{bipoles/interr/height 2/.initial=.1}
\ctikzset{bipoles/generic/height/.initial=.30}
\ctikzset{bipoles/generic/width/.initial=.80}
\ctikzset{bipoles/fuse/height/.initial=.20}
\ctikzset{bipoles/fuse/width/.initial=.50}
\ctikzset{bipoles/afuse/height/.initial=.20}
\ctikzset{bipoles/afuse/width/.initial=.50}
\ctikzset{bipoles/generic potentiometer/height/.initial=.80}
\ctikzset{bipoles/generic potentiometer/height 2/.initial=.30}
\ctikzset{bipoles/generic potentiometer/width/.initial=.80}
\ctikzset{bipoles/ageneric/height/.initial=.30}
\ctikzset{bipoles/ageneric/width/.initial=.80}
\ctikzset{bipoles/memristor/height/.initial=.30}
\ctikzset{bipoles/memristor/wave height/.initial=.5}
\ctikzset{bipoles/memristor/width/.initial=.80}
\ctikzset{bipoles/tgeneric/height/.initial=.70}
\ctikzset{bipoles/tgeneric/width/.initial=.80}
\ctikzset{bipoles/tfullgeneric/height/.initial=.70}
\ctikzset{bipoles/tfullgeneric/width/.initial=.80}
\ctikzset{bipoles/fullgeneric/height/.initial=.30}
\ctikzset{bipoles/fullgeneric/width/.initial=.80}
\ctikzset{bipoles/open/height/.initial=.25}
\ctikzset{bipoles/open/width/.initial=.8}
\ctikzset{bipoles/ammeter/height/.initial=.60}
\ctikzset{bipoles/ammeter/width/.initial=.60}
\ctikzset{bipoles/voltmeter/height/.initial=.60}
\ctikzset{bipoles/voltmeter/width/.initial=.60}
\ctikzset{bipoles/buffer/height/.initial=1}
\ctikzset{bipoles/buffer/width/.initial=1}
\ctikzset{bipoles/not port/width/.initial=1}
\ctikzset{bipoles/not port/height/.initial=.8}
\ctikzset{bipoles/not port/circle width/.initial=.15}
\ctikzset{bipoles/lamp/height/.initial=.60}
\ctikzset{bipoles/lamp/width/.initial=.60}
\ctikzset{bipoles/tline/height/.initial=.3}
\ctikzset{bipoles/tline/width/.initial=.8}
\ctikzset{bipoles/squid/height/.initial=.60}
\ctikzset{bipoles/squid/width/.initial=.60}
\ctikzset{bipoles/barrier/height/.initial=.60}
\ctikzset{bipoles/barrier/width/.initial=.60}
\ctikzset{bipoles/thermocouple/height/.initial=.250}
\ctikzset{bipoles/thermocouple/height 2/.initial=.60}
\ctikzset{bipoles/thermocouple/width/.initial=.140}
\ctikzset{bipoles/pushbutton/height/.initial=.5}
\ctikzset{bipoles/pushbutton/height 2/.initial=.0}
\ctikzset{bipoles/pushbutton/width/.initial=.50}

\newif\ifpgf@circuit@mos@arrows
\ctikzset{tripoles/mos style/.is choice}
\ctikzset{tripoles/mos style/no arrows/.code={\pgf@circuit@mos@arrowsfalse}}
\ctikzset{tripoles/mos style/arrows/.code={\pgf@circuit@mos@arrowstrue}}
\ctikzset{tripoles/nmos/width/.initial=.7}
\ctikzset{tripoles/nmos/gate height/.initial=.35}
\ctikzset{tripoles/nmos/base height/.initial=.5}
\ctikzset{tripoles/nmos/height/.initial=1.1}
\ctikzset{tripoles/nmos/base width/.initial=.5}
\ctikzset{tripoles/nmos/gate width/.initial=.62}
\ctikzset{tripoles/pmos/width/.initial=.7}
\ctikzset{tripoles/pmos/gate height/.initial=.35}
\ctikzset{tripoles/pmos/base height/.initial=.5}
\ctikzset{tripoles/pmos/height/.initial=1.1}
\ctikzset{tripoles/pmos/base width/.initial=.5}
\ctikzset{tripoles/pmos/gate width/.initial=.62}

\ctikzset{tripoles/nfet/width/.initial=.7}
\ctikzset{tripoles/nfet/gate height/.initial=.35}
\ctikzset{tripoles/nfet/base height/.initial=.5}
\ctikzset{tripoles/nfet/height/.initial=1.1}
\ctikzset{tripoles/nfet/base width/.initial=.5}
\ctikzset{tripoles/nfet/gate width/.initial=.62}

\ctikzset{tripoles/pfet/width/.initial=.7}
\ctikzset{tripoles/pfet/gate height/.initial=.35}
\ctikzset{tripoles/pfet/base height/.initial=.5}
\ctikzset{tripoles/pfet/height/.initial=1.1}
\ctikzset{tripoles/pfet/base width/.initial=.5}
\ctikzset{tripoles/pfet/gate width/.initial=.62}

\ctikzset{tripoles/nigfete/width/.initial=.7}
\ctikzset{tripoles/nigfete/gate height/.initial=.35}
\ctikzset{tripoles/nigfete/base height/.initial=.5}
\ctikzset{tripoles/nigfete/height/.initial=1.1}
\ctikzset{tripoles/nigfete/base width/.initial=.5}
\ctikzset{tripoles/nigfete/gate width/.initial=.62}

\ctikzset{tripoles/nigfetd/width/.initial=.7}
\ctikzset{tripoles/nigfetd/gate height/.initial=.35}
\ctikzset{tripoles/nigfetd/base height/.initial=.5}
\ctikzset{tripoles/nigfetd/height/.initial=1.1}
\ctikzset{tripoles/nigfetd/base width/.initial=.5}
\ctikzset{tripoles/nigfetd/gate width/.initial=.62}

\ctikzset{tripoles/pigfete/width/.initial=.7}
\ctikzset{tripoles/pigfete/gate height/.initial=.35}
\ctikzset{tripoles/pigfete/base height/.initial=.5}
\ctikzset{tripoles/pigfete/height/.initial=1.1}
\ctikzset{tripoles/pigfete/base width/.initial=.5}
\ctikzset{tripoles/pigfete/gate width/.initial=.62}

\ctikzset{tripoles/pigfetd/width/.initial=.7}
\ctikzset{tripoles/pigfetd/gate height/.initial=.35}
\ctikzset{tripoles/pigfetd/base height/.initial=.5}
\ctikzset{tripoles/pigfetd/height/.initial=1.1}
\ctikzset{tripoles/pigfetd/base width/.initial=.5}
\ctikzset{tripoles/pigfetd/gate width/.initial=.62}

\ctikzset{tripoles/npn/width/.initial=.6}
\ctikzset{tripoles/npn/gate height/.initial=.45}
\ctikzset{tripoles/npn/gate height 2/.initial=.15}
\ctikzset{tripoles/npn/base height/.initial=.4}
\ctikzset{tripoles/npn/height/.initial=1.1}
\ctikzset{tripoles/npn/gate width/.initial=.5}



\ctikzset{tripoles/pnp/width/.initial=.6}
\ctikzset{tripoles/pnp/gate height/.initial=.45}
\ctikzset{tripoles/pnp/gate height 2/.initial=.15}
\ctikzset{tripoles/pnp/base height/.initial=.4}
\ctikzset{tripoles/pnp/height/.initial=1.1}
\ctikzset{tripoles/pnp/gate width/.initial=.5}

\ctikzset{tripoles/pigbt/width/.initial=.6}
\ctikzset{tripoles/pigbt/gate height/.initial=.45}
\ctikzset{tripoles/pigbt/gate height 2/.initial=.15}
\ctikzset{tripoles/pigbt/base height/.initial=.4}
\ctikzset{tripoles/pigbt/height/.initial=1.1}
\ctikzset{tripoles/pigbt/gate width/.initial=.62}
\ctikzset{tripoles/pigbt/base width/.initial=.5}
\ctikzset{tripoles/nigbt/width/.initial=.6}
\ctikzset{tripoles/nigbt/gate height/.initial=.45}
\ctikzset{tripoles/nigbt/gate height 2/.initial=.15}
\ctikzset{tripoles/nigbt/base height/.initial=.4}
\ctikzset{tripoles/nigbt/height/.initial=1.1}
\ctikzset{tripoles/nigbt/gate width/.initial=.62}
\ctikzset{tripoles/nigbt/base width/.initial=.5}

\ctikzset{tripoles/njfet/width/.initial=.7}
\ctikzset{tripoles/njfet/gate height/.initial=.5}
\ctikzset{tripoles/njfet/gate height 2/.initial=.35}
\ctikzset{tripoles/njfet/gate width/.initial=.5}
\ctikzset{tripoles/njfet/height/.initial=1.1}
\ctikzset{tripoles/pjfet/width/.initial=.7}
\ctikzset{tripoles/pjfet/gate height/.initial=.5}
\ctikzset{tripoles/pjfet/gate height 2/.initial=.35}
\ctikzset{tripoles/pjfet/gate width/.initial=.5}
\ctikzset{tripoles/pjfet/height/.initial=1.1}

\ctikzset{tripoles/isfet/width/.initial=1}
\ctikzset{tripoles/isfet/gate height/.initial=.35}
\ctikzset{tripoles/isfet/base height/.initial=.5}
\ctikzset{tripoles/isfet/height/.initial=1.1}
\ctikzset{tripoles/isfet/base width/.initial=.3}
\ctikzset{tripoles/isfet/gate width/.initial=.5}
\ctikzset{tripoles/isfet/wave width/.initial=.16}
\ctikzset{tripoles/isfet/wave amp/.initial=.06}
\ctikzset{tripoles/isfet/waves y sep/.initial=.22}
\ctikzset{tripoles/isfet/waves x sep/.initial=.8}

\newif\ifpgf@circuit@europeanlogicport
\ctikzset{logic ports/.is choice}
\ctikzset{logic ports/european/.code= {\pgf@circuit@europeanlogicporttrue } }
\ctikzset{logic ports/american/.code= {\pgf@circuit@europeanlogicportfalse } } 

\newif\ifpgf@circuit@bipole@voltage@backward
\ctikzset{bipole/voltage/direction/.is choice}
\ctikzset{bipole/voltage/direction/forward/.code={\pgf@circuit@bipole@voltage@backwardfalse}}
\ctikzset{bipole/voltage/direction/backward/.code={\pgf@circuit@bipole@voltage@backwardtrue}}

\ctikzset{tripoles/american and port/width/.initial=1.1}
\ctikzset{tripoles/american and port/height/.initial=.8}
\ctikzset{tripoles/american and port/port width/.initial=.7}
\ctikzset{tripoles/american and port/input height/.initial=.5}
\ctikzset{tripoles/american nand port/width/.initial=1.1}
\ctikzset{tripoles/american nand port/height/.initial=.8}
\ctikzset{tripoles/american nand port/port width/.initial=.7}
\ctikzset{tripoles/american nand port/circle width/.initial=.15}
\ctikzset{tripoles/american nand port/input height/.initial=.5}
\ctikzset{tripoles/american or port/width/.initial=1.1}
\ctikzset{tripoles/american or port/height/.initial=.8}
\ctikzset{tripoles/american or port/port width/.initial=.7}
\ctikzset{tripoles/american or port/input height/.initial=.5}
\ctikzset{tripoles/american or port/input skip/.initial=.25}
\ctikzset{tripoles/american or port/aaa/.initial=.6}
\ctikzset{tripoles/american or port/bbb/.initial=.4} 
\ctikzset{tripoles/american or port/ccc/.initial=.5} 
\ctikzset{tripoles/american or port/ddd/.initial=.0}
\ctikzset{tripoles/american nor port/width/.initial=1.1}
\ctikzset{tripoles/american nor port/height/.initial=.8}
\ctikzset{tripoles/american nor port/port width/.initial=.7}
\ctikzset{tripoles/american nor port/input height/.initial=.5}
\ctikzset{tripoles/american nor port/input skip/.initial=.25}
\ctikzset{tripoles/american nor port/circle width/.initial=.15}
\ctikzset{tripoles/american nor port/aaa/.initial=.6}
\ctikzset{tripoles/american nor port/bbb/.initial=.4} 
\ctikzset{tripoles/american nor port/ccc/.initial=.5} 
\ctikzset{tripoles/american nor port/ddd/.initial=.0}
\ctikzset{tripoles/american xor port/width/.initial=1.1}
\ctikzset{tripoles/american xor port/height/.initial=.8}
\ctikzset{tripoles/american xor port/port width/.initial=.7}
\ctikzset{tripoles/american xor port/input height/.initial=.5}
\ctikzset{tripoles/american xor port/input skip/.initial=.15}
\ctikzset{tripoles/american xor port/distance/.initial=.1} 
\ctikzset{tripoles/american xor port/aaa/.initial=.6}
\ctikzset{tripoles/american xor port/bbb/.initial=.4} 
\ctikzset{tripoles/american xor port/ccc/.initial=.5} 
\ctikzset{tripoles/american xor port/ddd/.initial=.0}
\ctikzset{tripoles/american xnor port/width/.initial=1.1}
\ctikzset{tripoles/american xnor port/height/.initial=.8}
\ctikzset{tripoles/american xnor port/port width/.initial=.7}
\ctikzset{tripoles/american xnor port/input height/.initial=.5}
\ctikzset{tripoles/american xnor port/input skip/.initial=.15}
\ctikzset{tripoles/american xnor port/distance/.initial=.1} 
\ctikzset{tripoles/american xnor port/aaa/.initial=.6}
\ctikzset{tripoles/american xnor port/bbb/.initial=.4} 
\ctikzset{tripoles/american xnor port/ccc/.initial=.5} 
\ctikzset{tripoles/american xnor port/ddd/.initial=.0}
\ctikzset{tripoles/american xnor port/circle width/.initial=.15}
\ctikzset{tripoles/european and port/width/.initial=1.4}
\ctikzset{tripoles/european and port/height/.initial=.65}
\ctikzset{tripoles/european and port/reserved/.initial=.6}
\ctikzset{tripoles/european and port/input height/.initial=.6}
\ctikzset{tripoles/european or port/width/.initial=1.4}
\ctikzset{tripoles/european or port/height/.initial=.65}
\ctikzset{tripoles/european or port/reserved/.initial=.6}
\ctikzset{tripoles/european or port/input height/.initial=.6}
\ctikzset{tripoles/european xor port/width/.initial=1.4}
\ctikzset{tripoles/european xor port/height/.initial=.65}
\ctikzset{tripoles/european xor port/reserved/.initial=.6}
\ctikzset{tripoles/european xor port/input height/.initial=.6}
\ctikzset{tripoles/european nand port/width/.initial=1.4}
\ctikzset{tripoles/european nand port/not height/.initial=.3}
\ctikzset{tripoles/european nand port/not width/.initial=.8}
\ctikzset{tripoles/european nand port/height/.initial=.65}
\ctikzset{tripoles/european nand port/reserved/.initial=.6}
\ctikzset{tripoles/european nand port/input height/.initial=.6}
\ctikzset{tripoles/european not port/width/.initial=1.4}
\ctikzset{tripoles/european not port/not height/.initial=.3}
\ctikzset{tripoles/european not port/not width/.initial=.8}
\ctikzset{tripoles/european not port/height/.initial=.65}
\ctikzset{tripoles/european not port/reserved/.initial=.6}
\ctikzset{tripoles/european not port/input height/.initial=0}
\ctikzset{tripoles/european xnor port/width/.initial=1.4}
\ctikzset{tripoles/european xnor port/not height/.initial=.3}
\ctikzset{tripoles/european xnor port/not width/.initial=.8}
\ctikzset{tripoles/european xnor port/height/.initial=.65}
\ctikzset{tripoles/european xnor port/reserved/.initial=.6}
\ctikzset{tripoles/european xnor port/input height/.initial=.6}
\ctikzset{tripoles/european nor port/width/.initial=1.4}
\ctikzset{tripoles/european nor port/not height/.initial=.3}
\ctikzset{tripoles/european nor port/not width/.initial=.8}
\ctikzset{tripoles/european nor port/height/.initial=.65}
\ctikzset{tripoles/european nor port/reserved/.initial=.6}
\ctikzset{tripoles/european nor port/input height/.initial=.6}
\ctikzset{tripoles/op amp/width/.initial=1.7}
\ctikzset{tripoles/op amp/port width/.initial=.7}
\ctikzset{tripoles/op amp/height/.initial=1.4}
\ctikzset{tripoles/op amp/input height/.initial=.5}
\ctikzset{tripoles/op amp/up pos/.initial=.45}
\ctikzset{tripoles/plain amp/width/.initial=1.7}
\ctikzset{tripoles/plain amp/port width/.initial=.7}
\ctikzset{tripoles/plain amp/height/.initial=1.4}
\ctikzset{tripoles/plain amp/input height/.initial=.5}
\ctikzset{tripoles/plain amp/up pos/.initial=.45}

\ctikzset{tripoles/thyristor/height/.initial=1.10}
\ctikzset{tripoles/thyristor/height 2/.initial=.5}
\ctikzset{tripoles/thyristor/width/.initial=1.0}
\ctikzset{tripoles/thyristor/diode height/.initial=.5}
\ctikzset{tripoles/thyristor/diode width left/.initial=.4}
\ctikzset{tripoles/thyristor/diode width right/.initial=.3}

\ctikzset{tripoles/triac/height/.initial=1.1}
\ctikzset{tripoles/triac/width/.initial=1}
\ctikzset{tripoles/triac/diode width left/.initial=.3}
\ctikzset{tripoles/triac/diode width right/.initial=.3}

\ctikzset{tripoles/spdt/width/.initial=.85}
\ctikzset{tripoles/spdt/height/.initial=.45}
\ctikzset{tripoles/spdt/margin/.initial=.45}

\ctikzset{tripoles/toggleswitch/height/.initial=.8}
\ctikzset{tripoles/toggleswitch/height 2/.initial=.0}
\ctikzset{tripoles/toggleswitch/width/.initial=.80}

\ctikzset{tripoles/mixer/height/.initial=.85}
\ctikzset{tripoles/mixer/width/.initial=.85}
\ctikzset{tripoles/mixer/margin/.initial=.75}

\ctikzset{quadpoles/transformer/width/.initial=1.5}
\ctikzset{quadpoles/transformer/width1/.initial=.4}
\ctikzset{quadpoles/transformer/height/.initial=1.5}
\ctikzset{quadpoles/transformer/height1/.initial=.8}
\ctikzset{quadpoles/transformer core/width/.initial=1.5}
\ctikzset{quadpoles/transformer core/height/.initial=1.5}
\ctikzset{quadpoles/transformer core/core height/.initial=.5}
\ctikzset{quadpoles/transformer core/core width/.initial=.05}
\ctikzset{quadpoles/gyrator/width/.initial=1.5}
\ctikzset{quadpoles/gyrator/height/.initial=1.5}



\ctikzset{bipole/.is family}
\ctikzset{bipole/kind/.initial = }
\ctikzset{bipole/name/.initial = }
\newif\ifpgf@circuit@bipole@reversed
\ctikzset{bipole/reversed/.is if=pgf@circuit@bipole@reversed}
\newif\ifpgf@circuit@bipole@isvoltage
\ctikzset{bipole/is voltage/.is if=pgf@circuit@bipole@isvoltage}
\newif\ifpgf@circuit@bipole@iscurrent
\ctikzset{bipole/is current/.is if=pgf@circuit@bipole@iscurrent}

\ctikzset{bipole/voltage/.is family}
\newif\ifpgf@circuit@bipole@voltage@backward
\ctikzset{bipole/voltage/direction/.is choice}
\ctikzset{bipole/voltage/direction/forward/.code={\pgf@circuit@bipole@voltage@backwardfalse}}
\ctikzset{bipole/voltage/direction/backward/.code={\pgf@circuit@bipole@voltage@backwardtrue}}
\newif\ifpgf@circuit@bipole@voltage@below
\ctikzset{bipole/voltage/position/.is choice}
\ctikzset{bipole/voltage/position/above/.code={\pgf@circuit@bipole@voltage@belowfalse}}
\ctikzset{bipole/voltage/position/below/.code={\pgf@circuit@bipole@voltage@belowtrue}}

\ctikzset{bipole/voltage/label/unit/.initial=}
\ctikzset{bipole/voltage/label/name/.initial=}

\ctikzset{bipole/current/.is family}
\newif\ifpgf@circuit@bipole@current@backward
\ctikzset{bipole/current/direction/.is choice}
\ctikzset{bipole/current/direction/forward/.code={\pgf@circuit@bipole@current@backwardfalse}}
\ctikzset{bipole/current/direction/backward/.code={\pgf@circuit@bipole@current@backwardtrue}}
\newif\ifpgf@circuit@bipole@current@before
\ctikzset{bipole/current/x position/.is choice}
\ctikzset{bipole/current/x position/after/.code={\pgf@circuit@bipole@current@beforefalse}}
\ctikzset{bipole/current/x position/before/.code={\pgf@circuit@bipole@current@beforetrue}}
\newif\ifpgf@circuit@bipole@current@below
\ctikzset{bipole/current/y position/.is choice}
\ctikzset{bipole/current/y position/above/.code={\pgf@circuit@bipole@current@belowfalse}}
\ctikzset{bipole/current/y position/below/.code={\pgf@circuit@bipole@current@belowtrue}}

\ctikzset{bipole/current/label/unit/.initial=}
\ctikzset{bipole/current/label/name/.initial=}

\ctikzset{bipole/label/.is family}
\ctikzset{bipole/label/position/.initial=90}
\ctikzset{bipole/label/unit/.initial=}
\ctikzset{bipole/label/name/.initial=}
\ctikzset{bipole/nodes/.is family}
\ctikzset{bipole/nodes/left/.is choice}
\ctikzset{bipole/nodes/left/none/.code={\ctikzsetvalof{bipole/nodes/left}{none}}}
\ctikzset{bipole/nodes/left/empty/.code={\ctikzsetvalof{bipole/nodes/left}{empty}}}
\ctikzset{bipole/nodes/left/full/.code={\ctikzsetvalof{bipole/nodes/left}{full}}}
\ctikzset{bipole/nodes/right/.is choice}
\ctikzset{bipole/nodes/right/none/.code={\ctikzsetvalof{bipole/nodes/right}{none}}}
\ctikzset{bipole/nodes/right/empty/.code={\ctikzsetvalof{bipole/nodes/right}{empty}}}
\ctikzset{bipole/nodes/right/full/.code={\ctikzsetvalof{bipole/nodes/right}{full}}}


\newif\ifpgf@circuit@europeanresistor
\ctikzset{resistor/.is choice}
\ctikzset{resistor/american/.code = \pgf@circuit@europeanresistorfalse }
\ctikzset{resistor/european/.code = \pgf@circuit@europeanresistortrue }

\ctikzset{inductor/.is choice}
\ctikzset{inductor/cute/.code={\ctikzsetvalof{inductor}{cute}}}
\ctikzset{inductor/european/.code={\ctikzsetvalof{inductor}{european}}}
\ctikzset{inductor/american/.code={\ctikzsetvalof{inductor}{american}}}

\newif\ifpgf@circuit@fulldiode
\ctikzset{diode/.is if=pgf@circuit@fulldiode}
\ctikzset{diode/.is choice}
\ctikzset{diode/empty/.code = \pgf@circuit@fulldiodefalse }
\ctikzset{diode/full/.code = \pgf@circuit@fulldiodetrue }
\ctikzset{thickness/.initial=2}
\ctikzset{color/.initial=black}
\pgfkeys{/tikz/color/.add code={}{\ctikzset{color=#1}}}


\newif\ifpgf@circ@siunitx
\newif\ifpgf@circ@siunitx@res

\ctikzset{voltage/.is family}
\ctikzset{voltage/distance from node/.initial=.5} %\pgf@circ@Rlen units
\ctikzset{voltage/distance from line/.initial=.08} % pos, tra 0 e 1
\ctikzset{voltage/bump a/.initial=1.2}
\ctikzset{voltage/bump b/.initial=1.5}
\ctikzset{voltage/european label distance/.initial=1.4}
\ctikzset{voltage/american label distance/.initial=1.1}
% special cases
\ctikzset{bipoles/generic/voltage/distance from node/.initial=.4}
\ctikzset{bipoles/generic/voltage/bump b/.initial=2}
\ctikzset{bipoles/generic/voltage/european label distance/.initial=1.8}
%\ctikzset{bipoles/thermocouple/voltage/distance from node/.initial=.3}
\ctikzset{bipoles/thermocouple/voltage/bump b/.initial=2.2}
\ctikzset{bipoles/thermocouple/voltage/european label distance/.initial=1.5}
\ctikzset{bipoles/ageneric/voltage/distance from node/.initial=.4}
\ctikzset{bipoles/ageneric/voltage/bump b/.initial=2}
\ctikzset{bipoles/ageneric/voltage/european label distance/.initial=1.8}
\ctikzset{bipoles/fullgeneric/voltage/distance from node/.initial=.4}
\ctikzset{bipoles/fullgeneric/voltage/bump b/.initial=2}
\ctikzset{bipoles/fullgeneric/voltage/european label distance/.initial=1.8}
\ctikzset{bipoles/memristor/voltage/distance from node/.initial=.4}
\ctikzset{bipoles/memristor/voltage/bump b/.initial=2}
\ctikzset{bipoles/memristor/voltage/european label distance/.initial=1.8}
%\ctikzset{bipoles/tline/voltage/distance from node/.initial=.2}
\ctikzset{bipoles/tline/voltage/bump b/.initial=2.4}
\ctikzset{bipoles/tline/voltage/european label distance/.initial=2.1}
%\ctikzset{bipoles/varistor/voltage/distance from node/.initial=.2}
\ctikzset{bipoles/varistor/voltage/bump b/.initial=2.4}
\ctikzset{bipoles/varistor/voltage/european label distance/.initial=2}
%\ctikzset{bipoles/photoresistor/voltage/distance from node/.initial=.2}
\ctikzset{bipoles/photoresistor/voltage/bump b/.initial=2}
\ctikzset{bipoles/photoresistor/voltage/european label distance/.initial=1.8}
%\ctikzset{bipoles/thermistor/voltage/distance from node/.initial=.2}
\ctikzset{bipoles/thermistor/voltage/bump b/.initial=2.4}
\ctikzset{bipoles/thermistor/voltage/european label distance/.initial=2}
%\ctikzset{bipoles/thermistorntc/voltage/distance from node/.initial=.2}
\ctikzset{bipoles/thermistorntc/voltage/bump b/.initial=1.6}
%\ctikzset{bipoles/thermistorptc/voltage/distance from node/.initial=.2}
\ctikzset{bipoles/thermistorptc/voltage/bump b/.initial=1.6}

\ctikzset{current/.is family}
\ctikzset{current/distance/.initial = .5}

\tikzset{american currents/.style = { \circuitikzbasekey/current = american } }
\tikzset{european currents/.style = { \circuitikzbasekey/current = european } }
\tikzset{american voltages/.style = { \circuitikzbasekey/voltage = american } }
\tikzset{european voltages/.style = { \circuitikzbasekey/voltage = european } }
\tikzset{american resistors/.style = { \circuitikzbasekey/resistor = american } }
\tikzset{european resistors/.style = { \circuitikzbasekey/resistor = european } }
\tikzset{american inductors/.style = { \circuitikzbasekey/inductor = american } }
\tikzset{european inductors/.style = { \circuitikzbasekey/inductor = european } }
\tikzset{cute inductors/.style = { \circuitikzbasekey/inductor = cute } }
\tikzset{full diodes/.style = { \circuitikzbasekey/diode = full } }
\tikzset{empty diodes/.style = { \circuitikzbasekey/diode = empty } }
\tikzset{american ports/.style = { \circuitikzbasekey/logic ports = american } }
\tikzset{european ports/.style = { \circuitikzbasekey/logic ports = european } }
\tikzset{european/.style = { european currents, european voltages, european resistors, european inductors, european ports } }
\tikzset{american/.style = { american currents, american voltages, american resistors, american inductors, american ports } }
\tikzset{cute/.style = { european currents, european voltages, american resistors, cute inductors, american ports } }

% I should try to make the tree clearer (this voltaege conflicts with the options above)

\newif\ifpgf@circuit@europeanvoltage
\ctikzset{voltage/.is choice}
\ctikzset{voltage/american/.code = {\pgf@circuit@europeanvoltagefalse } }
\ctikzset{voltage/european/.code = {\pgf@circuit@europeanvoltagetrue } }

\newif\ifpgf@circuit@europeancurrent
\ctikzset{current/.is choice}
\ctikzset{current/american/.code = \pgf@circuit@europeancurrentfalse }
\ctikzset{current/european/.code = \pgf@circuit@europeancurrenttrue }

\ctikzset{label/align/.is choice}
\ctikzset{label/align/straight/.code={\ctikzsetvalof{label/align}{straight}}}
\ctikzset{label/align/rotate/.code={\ctikzsetvalof{label/align}{rotate}}}
\ctikzset{label/align/smart/.code={\ctikzsetvalof{label/align}{smart}}}
%% dependencies


\input pgfcircutils.sty
\input pgfcircmath.sty

\input pgfcircshapes.sty
\input pgfcircmonopoles.sty
\input pgfcircbipoles.sty
\input pgfcirctripoles.sty
\input pgfcircquadpoles.sty

\input pgfcirclabel.sty
\input pgfcircvoltage.sty
\input pgfcirccurrent.sty





